**采集卡2技术参数**

1.最大视频输入：1920x1080i@60/50fps

2.编码方式：Software Compression, Real-Time Modee

3.接口：USB3.0 Type B (SuperSpeed)UVC /USB2.0 Type B (High-Speed) UVC

4.视频输入接口：1xSDL，1xHDMI,1xDV-I,1xYPBPR,1xCVBS ,1 x S-Video

5.显示视频模式：YUY2

6.视频输入分辨率：USB2.0/3.0 Support Resolution

All resolution below

1920x1200p@60fps

7.录制视频模式：YUY2 (USB2.0/3.0)

8.录制视频分辨率：USB3.0 Support Resolution

1920x1200p@60150/30125/24fps

1920x1080p@60/50/30/25/24fps

1280x1024p@60/50130/25/24fps

1280x720p@60150130/25/24fps

1024x768p@60/50/30/25/24fps

800x600p@60/50/30/25/24fps

640x480p@60/50/30/25/24fps

720x576p@60/50/30/25/24fps

720x480p@60/50/30/25/24fps

USB2.0 Support Resolution

640x480p@30/25/24fps

720x576p@25/24fps

720x480p@25/24fps

9.音频输入：SDl Embedded Audio

HDMl Embedded Audio

2 x RCA (Audio L/R through component cable)

10.音频格式：Stereo/16-bit/48000Hz

11.操作系统：国产Kylin/Windows 7/Windows 8.1/Windows 10 ( 32-bit and 64-bit ) Linux/MAC OS /Android

满分50分，每有一条一般参数不响应扣 5分。